{"text_format":"1","workbook":"xlsx","n_sheets":5,"sheets":["ER","BLC","Limits","Transducers","Cable Attenuation"],"not_rendered":{"charts":0,"images":1,"macros":1,"external_links":0,"defined_names":8,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"ER","index":0,"n_rows":25,"n_cols":13,"rows_kept":25,"cut":false,"hidden":false,"merged":[[0,5,0,6],[1,5,1,6],[2,5,2,6],[3,5,3,6],[4,5,4,6],[0,1,0,3],[1,1,1,3],[2,1,2,3],[3,1,3,3],[4,1,4,3]]}
["EUT:","XYZ Widget",null,null,"Test ID:","ER-RS1A",null,"Combined Rd/RT?","No"]
["Test Date:","2017-02-23",null,null,"Red Signal #:","RS1A",null,"Test Type:","Rd"]
["Tested By:","John Doe",null,null,"Media (ER, BLC):","ER",null,"Category:","B"]
["Charge No.:","N/A",null,null,"Level (I, II, or III):","II",null,"Rd Rate:","1 kbps"]
["Mode:","EUT On in Mode A",null,null,"Signal Class:",2,null,"Rt Rate:","N/A"]
[]
[null,null,null,null,"Table of CE"]
[null,"Receiver","Signal","30% AM","Transducer",null,"Corrected",null,"Delta Above",null,"Lookup Table Parameters"]
["Frequency","Bandwidth","Generator","Factor","Correction Factor","Cable Loss","Level","Limit","Limit",null,"Transducer","Test Limit","Cable"]
["(MHz)","(MHz)","(dBm)","(dB)","(dB)","(dB)","(dBuV/m)","(dBuV/m)","(dB)",null,"(name)","(name)","(name)"]
[10,0.05,-82,-10,{"$f":"log_inter(A11,MATCH(K11,Transducer_No,0),Transducer)","v":6.1700000000000017},{"$f":"log_inter(A11,MATCH(M11,Cable_No,0),Cable)","v":0.1},{"$f":"C11+D11+E11+F11+107","v":21.269999999999996},{"$f":"log_inter(A11,MATCH(L11,Limit_No,0),Limit)+($F$5-2)*10","v":20},{"$f":"G11-H11","v":1.269999999999996},null,"SAS2A","ERIIB","Cable1"]
[62,0.05,-83,-10,{"$f":"log_inter(A12,MATCH(K12,Transducer_No,0),Transducer)","v":14.877585616720157},{"$f":"log_inter(A12,MATCH(M12,Cable_No,0),Cable)","v":0.25847833789965075},{"$f":"C12+D12+E12+F12+107","v":29.1360639546198},{"$f":"log_inter(A12,MATCH(L12,Limit_No,0),Limit)+($F$5-2)*10","v":35.84783378996508},{"$f":"G12-H12","v":-6.7117698353452795},null,"SAS2A","ERIIB","Cable1"]
[149,0.05,-87,-10,{"$f":"log_inter(A13,MATCH(K13,Transducer_No,0),Transducer)","v":7.1767226068749821},{"$f":"log_inter(A13,MATCH(M13,Cable_No,0),Cable)","v":0.37433206031929406},17.551054667194279,{"$f":"log_inter(A13,MATCH(L13,Limit_No,0),Limit)+($F$5-2)*10","v":43.463725368245477},-25.912670701051198,null,"SAS2A","ERIIB","Cable1"]
[225,0.05,-60,-10,{"$f":"log_inter(A14,MATCH(K14,Transducer_No,0),Transducer)","v":6.8118971366091481},{"$f":"log_inter(A14,MATCH(M14,Cable_No,0),Cable)","v":0.45115778184755528},44.263054918456703,{"$f":"log_inter(A14,MATCH(L14,Limit_No,0),Limit)+($F$5-2)*10","v":47.043650362227254},-2.7805954437705509,null,"SAS2A","ERIIB","Cable1"]
[]
[]
[]
[null,null,null,null,"Table of DRE"]
[null,"Receiver","Signal","30% AM","Transducer",null,"Corrected",null,"Delta Above",null,"Lookup Table Parameters"]
["Frequency","Bandwidth","Generator","Factor","Correction Factor","Cable Loss","Level","Limit","Limit",null,"Transducer","Test Limit","Cable"]
["(MHz)","(MHz)","(dBm)","(dB)","(dB)","(dB)","(dBuV/m)","(dBuV/m)","(dB)",null,"(name)","(name)","(name)"]
[25,0.05,-70,-10,{"$f":"log_inter(A22,MATCH(K22,Transducer_No,0),Transducer)","v":8.5},{"$f":"log_inter(A22,MATCH(M22,Cable_No,0),Cable)","v":0.17958800173440748},{"$f":"C22+D22+E22+F22+107","v":35.679588001734402},{"$f":"log_inter(A22,MATCH(L22,Limit_No,0),Limit)+($F$5-2)*10","v":27.95880017344075},{"$f":"G22-H22","v":7.720787828293652},null,"SAS2A","ERIIB","Cable1"]
[250,0.05,-83,-10,{"$f":"log_inter(A23,MATCH(K23,Transducer_No,0),Transducer)","v":4.8953056958512349},{"$f":"log_inter(A23,MATCH(M23,Cable_No,0),Cable)","v":0.470797032577982},{"$f":"C23+D23+E23+F23+107","v":19.366102728429212},{"$f":"log_inter(A23,MATCH(L23,Limit_No,0),Limit)+($F$5-2)*10","v":47.95880017344075},{"$f":"G23-H23","v":-28.592697445011538},null,"SAS2A","ERIIB","Cable1"]
[280,0.05,-87,-10,{"$f":"log_inter(A24,MATCH(K24,Transducer_No,0),Transducer)","v":7.5750949642179481},{"$f":"log_inter(A24,MATCH(M24,Cable_No,0),Cable)","v":0.4919215539586681},18.067016518176615,{"$f":"log_inter(A24,MATCH(L24,Limit_No,0),Limit)+($F$5-2)*10","v":48.943160626844382},-30.876144108667766,null,"SAS2A","ERIIB","Cable1"]
[300,0.05,-60,-10,{"$f":"log_inter(A25,MATCH(K25,Transducer_No,0),Transducer)","v":9.2065120772258915},{"$f":"log_inter(A25,MATCH(M25,Cable_No,0),Cable)","v":0.50478185834579559},46.711293935571689,{"$f":"log_inter(A25,MATCH(L25,Limit_No,0),Limit)+($F$5-2)*10","v":49.542425094393252},-2.8311311588215631,null,"SAS2A","ERIIB","Cable1"]

{"sheet":"BLC","index":1,"n_rows":25,"n_cols":13,"rows_kept":25,"cut":false,"hidden":false,"merged":[[3,1,3,3],[3,5,3,6],[4,1,4,3],[4,5,4,6],[0,1,0,3],[0,5,0,6],[1,1,1,3],[1,5,1,6],[2,1,2,3],[2,5,2,6]]}
["EUT:","XYZ Widget",null,null,"Test ID:","BLC-RS1A-CAN",null,"Combined Rd/RT?","No"]
["Test Date:","2017-02-23",null,null,"Red Signal #:","RS1A",null,"Test Type:","Rd"]
["Tested By:","John Doe",null,null,"Media (ER, BLC):","BLC-AC Neutral",null,"Category:","B"]
["Charge No.:","N/A",null,null,"Level (I, II, or III):","I",null,"Rd Rate:","500 bps"]
["Mode:","EUT On in Mode A",null,null,"Signal Class:",2,null,"Rt Rate:","N/A"]
[]
[null,null,null,null,"Table of CE"]
[null,"Receiver","Signal","30% AM","Transducer",null,"Corrected",null,"Delta Above",null,"Lookup Table Parameters"]
["Frequency","Bandwidth","Generator","Factor","Correction Factor","Cable Loss","Level","Limit","Limit",null,"Transducer","Test Limit","Cable"]
["(MHz)","(MHz)","(dBm)","(dB)","(dB)","(dB)","(dBuV)","(dBuV)","(dB)",null,"(name)","(name)","(name)"]
[10,0.05,-82,-10,{"$f":"log_inter(A11,MATCH(K11,Transducer_No,0),Transducer)","v":0},{"$f":"log_inter(A11,MATCH(M11,Cable_No,0),Cable)","v":0.1},{"$f":"C11+D11+E11+F11+107","v":15.099999999999994},{"$f":"log_inter(A11,MATCH(L11,Limit_No,0),Limit)+($F$5-2)*10","v":10},{"$f":"G11-H11","v":5.0999999999999943},null,"LISN7225-1","BLCIB","Cable1"]
[62,0.05,-83,-10,{"$f":"log_inter(A12,MATCH(K12,Transducer_No,0),Transducer)","v":0.15517006030607527},{"$f":"log_inter(A12,MATCH(M12,Cable_No,0),Cable)","v":0.25847833789965075},{"$f":"C12+D12+E12+F12+107","v":14.413648398205723},{"$f":"log_inter(A12,MATCH(L12,Limit_No,0),Limit)+($F$5-2)*10","v":21.88587534247381},{"$f":"G12-H12","v":-7.4722269442680869},null,"LISN7225-1","BLCIB","Cable1"]
[149,0.05,-87,-10,{"$f":"log_inter(A13,MATCH(K13,Transducer_No,0),Transducer)","v":0.78765616534371852},{"$f":"log_inter(A13,MATCH(M13,Cable_No,0),Cable)","v":0.37433206031929406},11.161988225663009,{"$f":"log_inter(A13,MATCH(L13,Limit_No,0),Limit)+($F$5-2)*10","v":27.597794026184111},-16.435805800521102,null,"LISN7225-1","BLCIB","Cable1"]
[225,0.05,-60,-10,{"$f":"log_inter(A14,MATCH(K14,Transducer_No,0),Transducer)","v":1.7},{"$f":"log_inter(A14,MATCH(M14,Cable_No,0),Cable)","v":0.45115778184755528},39.151157781847559,{"$f":"log_inter(A14,MATCH(L14,Limit_No,0),Limit)+($F$5-2)*10","v":30.282737771670437},8.8684200101771218,null,"LISNTH","BLCIB","Cable1"]
[]
[]
[]
[null,null,null,null,"Table of DRE"]
[null,"Receiver","Signal","30% AM","Transducer",null,"Corrected",null,"Delta Above",null,"Lookup Table Parameters"]
["Frequency","Bandwidth","Generator","Factor","Correction Factor","Cable Loss","Level","Limit","Limit",null,"Transducer","Test Limit","Cable"]
["(MHz)","(MHz)","(dBm)","(dB)","(dB)","(dB)","(dBuV)","(dBuV)","(dB)",null,"(name)","(name)","(name)"]
[25,0.05,-70,-10,{"$f":"log_inter(A22,MATCH(K22,Transducer_No,0),Transducer)","v":0},{"$f":"log_inter(A22,MATCH(M22,Cable_No,0),Cable)","v":0.17958800173440748},{"$f":"C22+D22+E22+F22+107","v":27.179588001734402},{"$f":"log_inter(A22,MATCH(L22,Limit_No,0),Limit)+($F$5-2)*10","v":15.969100130080562},{"$f":"G22-H22","v":11.210487871653839},null,"LISN7225-1","BLCIB","Cable1"]
[250,0.05,-83,-10,{"$f":"log_inter(A23,MATCH(K23,Transducer_No,0),Transducer)","v":1.7},{"$f":"log_inter(A23,MATCH(M23,Cable_No,0),Cable)","v":0.470797032577982},{"$f":"C23+D23+E23+F23+107","v":16.17079703257798},{"$f":"log_inter(A23,MATCH(L23,Limit_No,0),Limit)+($F$5-2)*10","v":30.969100130080562},{"$f":"G23-H23","v":-14.798303097502583},null,"LISNTH","BLCIB","Cable1"]
[280,0.05,-87,-10,{"$f":"log_inter(A24,MATCH(K24,Transducer_No,0),Transducer)","v":1.7},{"$f":"log_inter(A24,MATCH(M24,Cable_No,0),Cable)","v":0.4919215539586681},12.191921553958665,{"$f":"log_inter(A24,MATCH(L24,Limit_No,0),Limit)+($F$5-2)*10","v":31.707370470133288},-19.515448916174623,null,"LISNTH","BLCIB","Cable1"]
[300,0.05,-60,-10,{"$f":"log_inter(A25,MATCH(K25,Transducer_No,0),Transducer)","v":1.7},{"$f":"log_inter(A25,MATCH(M25,Cable_No,0),Cable)","v":0.50478185834579559},39.204781858345797,{"$f":"log_inter(A25,MATCH(L25,Limit_No,0),Limit)+($F$5-2)*10","v":32.156818820794939},7.0479630375508577,null,"LISNTH","BLCIB","Cable1"]

{"sheet":"Limits","index":2,"n_rows":8,"n_cols":17,"rows_kept":8,"cut":false,"hidden":false,"merged":[]}
["ER Level II Cat B (example only)",null,null,"ER Level II Cat C",null,null,"ER Level II Cat D",null,null,"ER Level II Cat E",null,null,"ER Level II Cat F",null,null,"BLC Level I Cat B"]
["Frequency","Level",null,"Frequency","Level",null,"Frequency","Level",null,"Frequency","Level",null,"Frequency","Level",null,"Frequency","Level"]
["(MHz)","(dBuV/m)",null,"(MHz)","(dBuV/m)",null,"(MHz)","(dBuV/m)",null,"(MHz)","(dBuV/m)",null,"(MHz)","(dBuV/m)",null,"(MHz)","(dBuV)"]
["ERIIB",null,null,"ERIIC",null,null,"ERIID",null,null,"ERIIE",null,null,"ERIIE",null,null,"BLCIB"]
[1E-3,80,null,1E-3,90,null,1E-3,100,null,1E-3,110,null,1E-3,120,null,1E-3,50]
[1,20,null,1,30,null,1,40,null,1,50,null,1,60,null,1,10]
[10,20,null,10,30,null,10,40,null,10,50,null,10,60,null,10,10]
[1000,60,null,1000,70,null,1000,80,null,1000,90,null,1000,100,null,1000,40]

{"sheet":"Transducers","index":3,"n_rows":52,"n_cols":29,"rows_kept":52,"cut":false,"hidden":false,"merged":[]}
["SAS-2/A","Antenna",null,"Rod","Antenna",null,"Bicon","Antenna",null,"LogPer","Antenna",null,"Horn3115","Antenna",null,"LISN7225-1",null,null,"LISN405-1AC",null,null,"LISN405-1DC",null,null,"LISN397-1-1",null,null,"LISNTH"]
["Antenna","Correction",null,"Antenna","Correction",null,"Antenna","Correction",null,"Antenna","Correction",null,"Antenna","Correction",null,"LISN","Correction",null,"LISN","Correction",null,"LISN","Correction",null,"LISN","Correction",null,"LISN","Correction"]
["Frequency","Factor",null,"Frequency","Factor",null,"Frequency","Factor",null,"Frequency","Factor",null,"Frequency","Factor",null,"Frequency","Factor",null,"Frequency","Factor",null,"Frequency","Factor",null,"Frequency","Factor",null,"Frequency","Factor"]
["(MHz)","(dB/m)",null,"(MHz)","(dB/m)",null,"(MHz)","(dB/m)",null,"(MHz)","(dB/m)",null,"(MHz)","(dB/m)",null,"(MHz)","(dB)",null,"(MHz)","(dB)",null,"(MHz)","(dB)",null,"(MHz)","(dB)",null,"(MHz)","(dB)"]
["SAS2A",null,null,"Rod",null,null,"Bicon",null,null,"LogPer",null,null,"Horn3115",null,null,"LISN7225-1",null,null,"LISN405-1AC",null,null,"LISN405-1DC",null,null,"LISN397-1-1",null,null,"LISNTH"]
[1E-4,51.11,null,8.9999999999999993E-3,8,null,20,10.9,null,200,15.8,null,1000,24.5,null,1E-4,34.715359195041707,null,1E-4,29.234339517267305,null,1E-4,0.41914060348711313,null,1,0.5,null,200,1.7]
[2.0000000000000001E-4,39.14,null,1,7.5,null,30,10.9,null,225,14.6,null,1500,25.5,null,2.0000000000000001E-4,28.699156214087953,null,2.0000000000000001E-4,23.229252601880987,null,2.0000000000000001E-4,0.10863807989205823,null,50,0.5,null,600,1.7]
[5.0000000000000001E-4,26.97,null,10,8.5,null,40,12.1,null,250,14.1,null,2000,27.9,null,4.0000000000000002E-4,22.696099648951687,null,4.0000000000000002E-4,17.270156423530672,null,4.0000000000000002E-4,0,null,100,1,null,700,1.4]
[1E-3,19.97,null,30,9,null,50,12.7,null,275,14.2,null,2500,28.7,null,1E-3,14.858157841354263,null,1E-3,9.7190946027057947,null,1E-3,0,null,200,2,null,800,1.1000000000000001]
[2E-3,14.36,null,null,null,null,60,11.1,null,300,15.4,null,3000,30.5,null,2E-3,9.2436521975865347,null,2E-3,4.9043838668473496,null,2E-3,0,null,null,null,null,900,0.8]
[5.0000000000000001E-3,9.4699999999999989,null,null,null,null,70,9.1,null,325,16.100000000000001,null,3500,31.7,null,4.0000000000000001E-3,4.5490818122305647,null,4.0000000000000001E-3,1.8280086732160763,null,4.0000000000000001E-3,0,null,null,null,null,1000,0.7]
[0.01,7.4200000000000017,null,null,null,null,80,7.8,null,350,17.399999999999999,null,4000,32.9,null,6.0000000000000001E-3,2.6064535555286179,null,6.0000000000000001E-3,0.90822806283323232,null,6.0000000000000001E-3,0,null,null,null,null,1500,1.2]
[0.02,6.2600000000000051,null,null,null,null,90,10.5,null,375,17.3,null,4500,32.6,null,8.0000000000000002E-3,1.6512672470433976,null,8.0000000000000002E-3,0.53400595977017562,null,8.0000000000000002E-3,0,null,null,null,null,2000,1]
[0.05,5.5300000000000011,null,null,null,null,100,12.5,null,400,17,null,5000,34.1,null,0.01,1.1262728227392247,null,0.01,0.34923763415880521,null,0.01,0,null,null,null,null,2500,0.6]
[0.1,5.3400000000000034,null,null,null,null,110,16.399999999999999,null,425,16.7,null,5500,34.700000000000003,null,1.4999999999999999E-2,0.53687222998049378,null,1.4999999999999999E-2,0,null,1.4999999999999999E-2,0,null,null,null,null,3000,1]
[0.2,5.1700000000000017,null,null,null,null,120,14.1,null,450,17.399999999999999,null,6000,35,null,0.05,0,null,4,0,null,4,0,null,null,null,null,3500,0.8]
[0.5,5.3400000000000034,null,null,null,null,130,13.9,null,475,18.7,null,6500,35.200000000000003,null,50,0,null,null,null,null,null,null,null,null,null,null,4000,0.8]
[1,5.3400000000000034,null,null,null,null,140,15.1,null,500,20.3,null,7000,36.5,null,100,0.5,null,null,null,null,null,null,null,null,null,null,4500,1.1000000000000001]
[2,5.3400000000000034,null,null,null,null,150,16.5,null,525,19.100000000000001,null,7500,37.4,null,200,1,null,null,null,null,null,null,null,null,null,null,5000,1.1000000000000001]
[5,6.6700000000000017,null,null,null,null,160,15.9,null,550,18.899999999999999,null,8000,37.200000000000003,null,null,null,null,null,null,null,null,null,null,null,null,null,5500,1.1000000000000001]
[10,6.1700000000000017,null,null,null,null,170,17.100000000000001,null,575,19.2,null,8500,37.799999999999997,null,null,null,null,null,null,null,null,null,null,null,null,null,6000,1.3]
[15,7,null,null,null,null,180,16.7,null,600,19.600000000000001,null,9000,38.1,null,null,null,null,null,null,null,null,null,null,null,null,null,6500,1.3]
[20,7.5,null,null,null,null,190,18.899999999999999,null,625,20.5,null,9500,38.200000000000003,null,null,null,null,null,null,null,null,null,null,null,null,null,7000,1.2]
[25,8.5,null,null,null,null,200,18,null,650,21.6,null,10000,38.299999999999997,null,null,null,null,null,null,null,null,null,null,null,null,null,7500,1.3]
[30,9.8299999999999983,null,null,null,null,null,null,null,675,21.8,null,10500,38.4,null,null,null,null,null,null,null,null,null,null,null,null,null,8000,2.2000000000000002]
[30,10.566230399979835,null,null,null,null,null,null,null,700,21.1,null,11000,38.9,null,null,null,null,null,null,null,null,null,null,null,null,null,8500,2.7]
[35,16.948537041403149,null,null,null,null,null,null,null,725,21,null,11500,39.6,null,null,null,null,null,null,null,null,null,null,null,null,null,9000,2.6]
[40,16.638388456980817,null,null,null,null,null,null,null,750,21.5,null,12000,39.200000000000003,null,null,null,null,null,null,null,null,null,null,null,null,null,9500,4]
[45,14.512686813778817,null,null,null,null,null,null,null,757,22.1,null,12500,39,null,null,null,null,null,null,null,null,null,null,null,null,null,10000,4.2]
[49.9,14.235888116145979,null,null,null,null,null,null,null,800,22.6,null,13000,40]
[50,14.284240296045766,null,null,null,null,null,null,null,825,22.6,null,13500,40.6]
[60,15.187786002371645,null,null,null,null,null,null,null,850,22.7,null,14000,41.3]
[70,13.729479850826156,null,null,null,null,null,null,null,875,22.9,null,14500,41]
[80,13.86301565361083,null,null,null,null,null,null,null,900,23.3,null,15000,39.6]
[90,11.654919601229242,null,null,null,null,null,null,null,925,23.7,null,15500,38.299999999999997]
[100,10.198067321777355,null,null,null,null,null,null,null,950,23.9,null,16000,38.799999999999997]
[120,7.8663957429469846,null,null,null,null,null,null,null,975,24,null,16500,40.5]
[139.9,7.3127164820764499,null,null,null,null,null,null,null,1000,24.4,null,17000,41.5]
[140,7.3117204202589576,null,null,null,null,null,null,null,null,null,null,17500,44.3]
[160,7.0223894017545803,null,null,null,null,null,null,null,null,null,null,18000,48.5]
[180,8.1033611899491014]
[200,8.9544640801749935]
[250,4.8953056958512349]
[300,9.2065120772258915]
[399.9,9.5012681917258313]
[400,9.307847227732772]
[500,11.655658295313312]
[600,12.287825675223186]
[700,17.378826011714853]
[800,16.009400846481977]
[900,22.47674806192256]
[1000,20.209103240966819]

{"sheet":"Cable Attenuation","index":4,"n_rows":13,"n_cols":17,"rows_kept":13,"cut":false,"hidden":false,"merged":[]}
["Cable",null,null,"Cable",null,null,"Cable",null,null,"Cable",null,null,"Cable",null,null,"Cable"]
["Loss",null,null,"Loss",null,null,"Loss",null,null,"Loss",null,null,"Loss",null,null,"Loss"]
["Frequency","Loss",null,"Frequency","Loss",null,"Frequency","Loss",null,"Frequency","Loss",null,"Frequency","Loss",null,"Frequency","Loss"]
["(MHz)","(dB)",null,"(MHz)","(dB)",null,"(MHz)","(dB)",null,"(MHz)","(dB)",null,"(MHz)","(dB)",null,"(MHz)","(dB)"]
["Cable1",null,null,"Cable2",null,null,"Cable3",null,null,"Cable4",null,null,"Cable5",null,null,"Cable6"]
[1E-4,0,null,1E-4,0,null,1E-4,0,null,1E-4,0,null,1E-4,0,null,1E-4,0]
[10,0.1,null,10,0.11000000000000001,null,10,0.12,null,10,0.13,null,10,0.13999999999999999,null,10,0.13999999999999999]
[100,0.3,null,100,0.33,null,100,0.36,null,100,0.39,null,100,0.42,null,100,0.42]
[500,0.6,null,500,0.66,null,500,0.72,null,500,0.78,null,500,0.84,null,500,0.84]
[1000,2,null,1000,2.2000000000000002,null,1000,2.4,null,1000,2.6,null,1000,2.8,null,1000,2.8]
[3000,3,null,3000,3.3000000000000003,null,3000,3.5999999999999996,null,3000,3.9000000000000004,null,3000,4.1999999999999993,null,3000,4.1999999999999993]
[6000,4,null,6000,4.4000000000000004,null,6000,4.8,null,6000,5.2,null,6000,5.6,null,6000,5.6]
[10000,6,null,10000,6.6000000000000005,null,10000,7.1999999999999993,null,10000,7.8000000000000007,null,10000,8.3999999999999986,null,10000,8.3999999999999986]